**Lessons Learned**

## Event Summary

## Contributing Factors

* - Equipment tethers not being utilized inside the piers
* - Water pump not adequately secured on the platform pier
* - False sense of security regarding prevention measures
* - Clutter and tools in a tight work location
* - Power cord tension causing the pump to tip over

## Lessons Learned

* - Implement a process flow to prevent dropped objects by securing or barricading loose items
* - Regularly verify compliance with safety absolutes and conduct monthly drop object blitzes
* - Ensure proper head protection is worn by all workers
* - Visually assess tasks to prevent entanglement with surrounding objects
* - Remove unnecessary tools and equipment immediately after use
* - Follow and verify all dropped object prevention SOPs and requirements

Contact for Further Information

Name: Rob Covassin

Email Address: rcovassin@aecon.com